DucoDoor Wall

Manufactured by: DUCO 'Ventilation & Sun Control'

DucoDoor Wall is a louvre door with the same louvres and profiles as the louvre wall.

DucoDoor Wall and the wall thus form a perfect unit, as the door is fully integrated into the wall.

## Features:

* Louvre type: Choice among almost the entire DucoWall range, details on request
* Door type: Both single and double doors possible
* Direction of pivot: Outward or inward opening (reinforced only possible with outward opening doors)
* Version: Left or right
* Useful height (UH):
	+ Maximum UH: 3000 mm
* Useful width (UW):
	+ Maximum UW single door: 1500 mm
	+ Maximum UW double door: 3000 mm
* Hinges: Duco Pivot system top and bottom (hinge plate thickness: 8 mm)
* Lock height (LH):
	+ Standard LH: 1064 mm
	+ Depending on louvre step, adaptable on customer demand.
* Frame profile: 50/50
* Mullion:
	+ 40/21 for DucoWall Screening louvres
	+ 40/21 for DucoWall Solid louvres
	+ All others with Duco clips.
* Hand protection:
	+ Lock plate on the lock side of the door.
	+ Lock shield opposite the lock plate.
* Door furniture:
	+ Standard: T-handle (outside) + door handle (inside)

 Cylinder lock (with 3 keys) 60mm Type 30/30

* + Optional: Panic lock - Outdoor module + Knob

Panic lock - Outdoor module (without knob)

 Cylinder lock 40mm Type 30/10

* + Other combinations available on request.
* Visual free area: Idem selected louvre wall
* Physical free area: Idem selected louvre wall
* Material:
	+ Aluminium: Al Mg Si 0.5
	+ Plastic: Polyamide PA 6.6 - glass-fibre reinforced

## Surface treatment:

* Anodised in natural as standard (15-20 µm)
* Enamelled polyester powder coating (60-80 µm)
* Specific RAL codes and/or textured paint on request

## Functional specifications:

### Flow rate:

* + K-factor intake: dependent on louvre
	+ K-factor exhaust: dependent on louvre